Symobi for Peagsos/ODW
======================

The enclosed ISO image contains a Symobi LiveCD for Pegasos/ODW. Please keep in mind that
this is only a demo, showing a smoothly running Symobi and some testing applications. By the
following steps, you can easily run this live demo of Symobi on your Pegasos/ODW:

- create a CD from the ISO image
- when turning on the Pegasos/ODW, use <Esc> to enter the firmware console
- insert the CD into the CD drive
- use 'printenv boot-device' and note down your current boot device
- use 'setenv boot-device cd' to enable booting from CD
- use 'printenv boot-file' and note down your current boot device
- use 'setenv boot-file kernel.fth' to tell OF which file to boot
- enter 'boot' to - well - boot....
...
- enjoy the Symobi demo
...
- afterwards you may want to use the 'setenv' command to restore your original values
  for 'boot-device' and 'boot-file'


IMPORTANT NOTE
--------------
The version of Symobi on this LiveCD contains some preliminary code parts for graphic
initialization. It has been developed and tested on an ODW with SmartFirmware version
1.2 (20040810112413) and an ATI Radeon 9250. There is a chance, but no kind of surety
that this LiveCD runs with other versions of the ODW, too. Thus, we recommend to run
it only if your ODW has the same firmware version and the same graphics card installed.